\hypertarget{ads1110_8c}{
\section{ads1110.c File Reference}
\label{ads1110_8c}\index{ads1110.c@{ads1110.c}}
}
{\tt \#include \char`\"{}ads1110.h\char`\"{}}\par
\subsection*{Functions}
\begin{CompactItemize}
\item 
uint8\_\-t \hyperlink{ads1110_8c_92b2b1671aa9b65a62976819b896c82e}{read\_\-ads1110} (uint8\_\-t $\ast$dataloc)
\begin{CompactList}\small\item\em reads 2 bytes of data from an ADS1110 via I2C \item\end{CompactList}\end{CompactItemize}


\subsection{Function Documentation}
\hypertarget{ads1110_8c_92b2b1671aa9b65a62976819b896c82e}{
\index{ads1110.c@{ads1110.c}!read\_\-ads1110@{read\_\-ads1110}}
\index{read\_\-ads1110@{read\_\-ads1110}!ads1110.c@{ads1110.c}}
\subsubsection[{read\_\-ads1110}]{\setlength{\rightskip}{0pt plus 5cm}uint8\_\-t read\_\-ads1110 (uint8\_\-t $\ast$ {\em dataloc})}}
\label{ads1110_8c_92b2b1671aa9b65a62976819b896c82e}


reads 2 bytes of data from an ADS1110 via I2C 

\begin{Desc}
\item[Parameters:]
\begin{description}
\item[{\em $\ast$dataloc}]Pointer to location in which to store data \end{description}
\end{Desc}
\begin{Desc}
\item[Returns:]errorcode value returned by read from I2C function.\end{Desc}
Currently, errorcode is always zero requires the i2c library 